¡Ü firmware V4.50-B0
1. Default IP setting changed from DHCP to Static (10.20.30.40)
2. Delete of FCM Push function
3. Delete of RTP Start Port Menu from RTP/RTSP Menu
4. Add Modbus function
5. In the Stream Setup Menu, Default of Video With Flexible Extra System Data is set to Enable.
   - This setting is changed to support AI.

---------------------------------------------------------------------------------------

¡Ü Firmware V4.48-B1 Release Note
1. Corrected the aspect ratio menu at 5M camera
2. Added S/W watch-dog funciton(encoding)
3. Optimized ¡°Advanced Service¡± functions

---------------------------------------------------------------------------------------

¡Ü Firmware V4.48-B0 Release Note
1. Adds Text OSD features and stabilize (Dome, Bullet, PTZ camera)
2. Adds PTZ Text OSD (PTZ Camera)
3. Add Korea Expressway Corporation protocol ( Subtitle and Controller feature added as an option )
4. Supports AAC-LC Audio CODEC
5. Adds IR Control feature for Global Shutter Camera
6. Adds Audio Detection features
 - Adds control features for Mic Volume.
 - Adds setting features for Detection Threshold.
7. Adds Night Mode / DI Mode / Motion Mode. ( Excludes GSM, HSM, PTZ Camera)
   A. Function to temporarily change settings when an event occurs unlike Day and Night.
8. Adds setting and change function of Color Mode  ( Excludes GSM, HSM, PTZ Camera)
   A. Adjust of the camera¡¯s default color setting level
   B. Select option of Default / Standard / Vivid Mode
9. Change of the default GOP setting ( 30 to 60 )
10. Stabilize of IP-CCTV DNS interface protocol

---------------------------------------------------------------------------------------

¡Ü Rev-A firmware ver4.46-B10
1. Add On Service featue added
   POS features which was supported by previous TI platform are now included in Rev-A Camera models using Ambarella chipset
2. Improvement of motion detection sensitivity and default motion detection area setup has been changed
   After firmware upgrade, the previously saved motion detection area is maintained.
   To restore the default motion detection area ( Upper Left, Upper Right, Lower Left and Lower Right ), 
    run ¡°Restore Default¡± from the Utility menu at Admin Page.


---------------------------------------------------------------------------------------

¡Ü Rev-A firmware ver4.46-B3
1. Supports Corridor format.
2. Fixed bug that motion detection did not end when disables motion detection while motion is being detected.

---------------------------------------------------------------------------------------

¡Ü Rev-A firmware ver4.46-B0
1. The initial release firmware for Rev-A Camera using Ambarella chipset
2. Add ¡°Management White List¡± function
3. Add ¡°Role¡± option on User Registration Screen ( User, Manager, Administrator )
4. Add ¡°FCM (Firebase Cloud Messaging) Push Service¡± function
   - Can be used in conjunction with FlexWATCH Mobile App
5. The detection protocol version upgraded ( Effective when using IP Installer v3.11.0 )
   - Supports more than 11 digits of Model number
6. RTSP streaming performance and functionality improved
   - RTSP streaming performance improved
   - Supports SHA256 encryption
7. Log function upgraded
   - Log will remain even if Camera rebooted
   - Strengthening Log lists
   - Log page displayed as 8 Split
8. Stabilizing HTTPS functionality
9. Built-in Smart Viewer V1.21.0.0 / Smart Player V1.12.0.0
